|  |
| --- |
| **PRODUCT DATA SHEET****HPMA** |
| Synonyms | Hydrolyzed Polymaleic Anhydride |
| CAS Number | 26099-09-02 |
| UN No. | 3265 |
| Structural Formula | http://www.th-chem.com/cp_img/3/HPMA.gif |
| Product Grade | Industrial |
| Description & Application | HPMA is a low molecular weight polymeride, with average molecular weight 400-800. No toxicity, soluble in water, high chemical and thermal stability, decomposed temperature above 330℃. HPMA has obvious threshold effect under high temperature (350℃) and high pH(8.3)level, suitable to be used in alkaline water system or built with agents. It has good scale inhibition against carbonate and phosphate scales under temperature 300℃ with effective time as long as 100 hours. Due to its good scale inhibition and high temperature tolerance properties, HPMA is widely used in desalination plant of flash vaporization equipment, low pressure boiler, steam locomotive, crude oil evaporation, petroleum pipeline, and industrial circulating cool water systems. In addition, HPMA has good corrosion inhibition effect when used together with zinc salt. HPMA can also used as additives for cement.  |
| Safety Protection | Acidity, avoid contact with eye and skin, once contacted, flush with water. |
| Specification | Solid content% : ≥48Bromine value(mg/g)：≤80.0pH（1% solution）: 2.0-3.0Density(20℃) g/cm3 : ≥1.180Appearance: Pale yellow to umber transparent liquid  |
| Package  | Normally In 25kg net Plastic Drum. Stored in cool and dry place.  |
| Shelf Life | 10 Months. |